Par Statistics
Total Non-vccgnd Signals=640
Total Non-vccgnd Design Pins=2054
Total Non-vccgnd Conns=2054
Total Non-vccgnd Timing Constrained Conns=1809
Phase 1 CPU=4.7 sec
Phase 2 CPU=5.1 sec
Phase 3 CPU=6.6 sec
Phase 4 CPU=7.1 sec
Phase 5 CPU=9.0 sec
Phase 6 CPU=9.3 sec
Phase 7 CPU=15.3 sec
Phase 8 CPU=15.3 sec
Phase 9 CPU=15.3 sec
Phase 10 CPU=15.3 sec
Phase 11 CPU=15.5 sec
AvgWirelenPerPin Fanout 1=3.0
AvgWirelenPerPin Fanout 2=2.5
AvgWirelenPerPin Fanout 3=1.7
AvgWirelenPerPin Fanout 4=1.8
AvgWirelenPerPin Fanout 10=3.2
AvgWirelenPerPin Fanout 50=1.9
AvgWirelenPerPin Fanout 100=9.2
AvgWirelenPerPin Fanout 500=0.0
AvgWirelenPerPin Fanout 5000=0.0
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=1.9293